From 00a3fc7ec097da17080914af76ca7f3b90a965f2 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Nils=20Wallm=C3=A9nius?= <nils@rockbox.org>
Date: Fri, 19 Jan 2007 12:42:19 +0000
Subject: Make changes to the gigabeat manual suggested by Alison Gravley and
 some other minor tweaks

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@12072 a1c6a512-1295-4272-9138-f99709370657
---
 manual/configure_rockbox/system_options.tex | 10 +++++-----
 1 file changed, 5 insertions(+), 5 deletions(-)

(limited to 'manual/configure_rockbox/system_options.tex')

diff --git a/manual/configure_rockbox/system_options.tex b/manual/configure_rockbox/system_options.tex
index da24ff8..1d8bfdc 100644
--- a/manual/configure_rockbox/system_options.tex
+++ b/manual/configure_rockbox/system_options.tex
@@ -124,20 +124,20 @@ This sub menu relates to limits in the Rockbox operating system.
       This option turns \setting{On} and \setting{Off} the car ignition
       auto stop function.
   \begin{description}
-  \item [Car Adapter Mode: ]When using the \dap\ in a car,
-  \setting{Car Adapter Mode} automatically stops playback on the \dap\ when
+  \item [Car Adapter Mode: ]When using the \dap{} in a car,
+  \setting{Car Adapter Mode} automatically stops playback on the \dap{} when
   power (i.e. from cigarette lighter power adapter) to the external DC in jack
   is turned off. If the \setting{Car Adapter Mode} is set to \setting{On},
   Rockbox will pause playback when the external power off condition is
-  detected. Rockbox will then shutdown the \dap\ after the length of time set
+  detected. Rockbox will then shutdown the \dap{} after the length of time set
   in the \setting{Idle Poweroff} setting (see above).
   If power to the DC in jack is turned back on before the \emph{Idle Poweroff}
-  function has shut the \dap\ off, playback will be resumed 5 seconds after
+  function has shut the \dap{} off, playback will be resumed 5 seconds after
   the power is applied. This delay is to allow for the time while the car
   engine is being started.
   \end{description}
 
-  Once the \dap\ is shut off either manually, or automatically with the
+  Once the \dap{} is shut off either manually, or automatically with the
   \setting{Idle Poweroff} function, it must be powered up manually to resume
   playback.
 }
-- 
cgit v1.1

