From 2391ad73d0fdca7b2cbe3305cd4d616875bb83e1 Mon Sep 17 00:00:00 2001
From: Marc Guay <marcguay@rockbox.org>
Date: Tue, 7 Oct 2008 00:31:51 +0000
Subject: Change UMS to MSC in the Sansa e200 uninstallation instructions, as
 it is referred to as such both by the installation instructions and the OF.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@18724 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 7ad2037..70e44c8 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -429,7 +429,7 @@ completely follow the manual uninstallation instructions below.}}
   connect the \dap{} to your computer, and follow the instructions to install
   the bootloader, but when prompted by sansapatcher, enter \texttt{u} for uninstall,
   instead of \texttt{i} for install. As in the installation, it may be necessary to
-  first put your device into UMS mode.
+  first put your device into MSC mode.
 }
 
 \optv{ipod}{
-- 
cgit v1.1

