From 5c826ca912d87f568b042de6bab2cb15f53d74ef Mon Sep 17 00:00:00 2001
From: Alex Parker <rockbox@aeparker.com>
Date: Sat, 21 Nov 2009 18:06:23 +0000
Subject: The Clip has no recovery mode.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@23683 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/installation.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/getting_started/installation.tex')

diff --git a/manual/getting_started/installation.tex b/manual/getting_started/installation.tex
index 6a22bbd..7cd66b8 100644
--- a/manual/getting_started/installation.tex
+++ b/manual/getting_started/installation.tex
@@ -111,7 +111,7 @@ follow the instructions at
     \setting{Settings $\rightarrow$ USB Mode} to \setting{MSC} from within the
     original firmware.}
 
-    \nopt{e200v2,clip}{\warn{Never extract files to your \dap{} while it is in recovery mode.}}
+    \nopt{e200v2}{\warn{Never extract files to your \dap{} while it is in recovery mode.}}
   }
   \opt{h10,h10_5gb}{
     The installation requires you to use UMS mode and so
-- 
cgit v1.1

