From 0fdc2d55412bb57341eb9ee852a82b3eec2854d9 Mon Sep 17 00:00:00 2001
From: Dave Chapman <dave@dchapman.com>
Date: Thu, 25 Mar 2010 20:11:34 +0000
Subject: Initial manuals for clipv2 and clip+, with corrected installation
 instructions.  The player picture in Chapter 3 is the same as the Clipv1 for
 both Clipv2 and Clip+ - this needs changing for the Clip+.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25332 a1c6a512-1295-4272-9138-f99709370657
---
 manual/getting_started/sansaAMS_install.tex | 22 ++++++++++++++++------
 1 file changed, 16 insertions(+), 6 deletions(-)

(limited to 'manual/getting_started/sansaAMS_install.tex')

diff --git a/manual/getting_started/sansaAMS_install.tex b/manual/getting_started/sansaAMS_install.tex
index 7ef2eed..44bfa2c 100644
--- a/manual/getting_started/sansaAMS_install.tex
+++ b/manual/getting_started/sansaAMS_install.tex
@@ -9,13 +9,17 @@ files:
       \url{http://forums.sandisk.com/sansa/board/message?board.id=e200&thread.id=13548}}
     \opt{fuze}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=sansafuse&thread.id=23276}}
-    \opt{clip}{
+    \opt{clipv1,clipv2}{
       \url{http://forums.sandisk.com/sansa/board/message?board.id=clip&thread.id=15109}}
+    \opt{clipplus}{
+      \url{http://forums.sandisk.com/sansa/board/message?board.id=clipplus&thread.id=2911}}
 
   \item The bootloader: 
     \opt{e200v2}{\download{bootloader/sandisk-sansa/e200v2/bootloader-e200v2.sansa}}
     \opt{fuze}{\download{bootloader/sandisk-sansa/fuze/bootloader-fuze.sansa}}
-    \opt{clip}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}
+    \opt{clipv1}{\download{bootloader/sandisk-sansa/clip/bootloader-clip.sansa}}
+    \opt{clipv2}{\download{bootloader/sandisk-sansa/clipv2/bootloader-clipv2.sansa}}
+    \opt{clipplus}{\download{bootloader/sandisk-sansa/clipplus/bootloader-clipplus.sansa}}
 
   \item The version of mkamsboot for your operating system from
     \download{bootloader/sandisk-sansa/mkamsboot/}
@@ -36,7 +40,9 @@ files:
   \begin{code} 
     \opt{fuze}{mkamsboot.exe fuzea.bin bootloader-fuze.sansa patched.bin}
     \opt{e200v2}{mkamsboot.exe e200pe.bin bootloader-e200v2.sansa patched.bin}
-    \opt{clip}{mkamsboot.exe m300a.bin bootloader-clip.sansa patched.bin}
+    \opt{clipv1}{mkamsboot.exe m300a.bin bootloader-clip.sansa patched.bin}
+    \opt{clipv2}{mkamsboot.exe m30pa.bin bootloader-clipv2.sansa patched.bin}
+    \opt{clipplus}{mkamsboot.exe clppa.bin bootloader-clipplus.sansa patched.bin}
   \end{code}
  
   If mkamsboot.exe does not report success, then retry or abort.
@@ -44,7 +50,8 @@ files:
 \item Copy the output file (``patched.bin'' in the example given above) to the
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
-  \opt{clip}{(``m300a.bin''} above).
+  \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
+  \opt{clipplus}{(``clppa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
@@ -64,7 +71,9 @@ files:
   \begin{code} 
     \opt{fuze}{./mkamsboot fuzea.bin bootloader-fuze.sansa patched.bin}
     \opt{e200v2}{./mkamsboot e200pe.bin bootloader-e200v2.sansa patched.bin}
-    \opt{clip}{./mkamsboot m300a.bin bootloader-clip.sansa patched.bin}
+    \opt{clipv1}{./mkamsboot m300a.bin bootloader-clip.sansa patched.bin}
+    \opt{clipv2}{./mkamsboot m30pa.bin bootloader-clipv2.sansa patched.bin}
+    \opt{clipplus}{./mkamsboot clppa.bin bootloader-clipplus.sansa patched.bin}
   \end{code}
  
   If mkamsboot does not report success, then retry or abort.
@@ -72,7 +81,8 @@ files:
 \item Copy the output file (``patched.bin'' in the example given above) to the
   root of the device and rename it to the same name as the OF file you downloaded earlier 
   \opt{fuze}{(``fuzea.bin''} \opt{e200v2}{(``e200pe.bin''}
-  \opt{clip}{(``m300a.bin''} above).
+  \opt{clipv1}{(``m300a.bin''} \opt{clipv2}{(``m30pa.bin''}
+  \opt{clipplus}{(``clppa.bin''} above).
 
 \item Safely eject the device, unplug USB and wait for the firmware update to finish.
 \end{enumerate}
-- 
cgit v1.1

