From 10d0344e296eeb9259e9b609bb9b656ba1d7e42a Mon Sep 17 00:00:00 2001
From: Thom Johansen <thomj@rockbox.org>
Date: Thu, 13 Dec 2007 22:51:27 +0000
Subject: FS #8315 and FS #8316, plus some of my own small changes. Pretty much
 just minor language rewrites.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@15919 a1c6a512-1295-4272-9138-f99709370657
---
 manual/plugins/alpinecdc.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/plugins/alpinecdc.tex')

diff --git a/manual/plugins/alpinecdc.tex b/manual/plugins/alpinecdc.tex
index d493c55..008bb62 100644
--- a/manual/plugins/alpinecdc.tex
+++ b/manual/plugins/alpinecdc.tex
@@ -15,7 +15,7 @@ M-Bus radios have a DIN-style circular jack with 8 pins (7 in a $\sim$ 270 degre
 circle, one in the center). A standard 5-pin DIN plug is OK for this, since we
 don't use the other (power) pins.
 
-As OEM, they shuffled the pins around a bit, better check first if it's not
+As OEM, they shuffled the pins around a bit, better check first if it is not
 genuine Alpine. The bus pin is pulled high to 12 volts with a $\sim$ 2kOhm resistor,
 pulses driven low. Because it's open collector, this is not harmful to the
 Archos.\\
-- 
cgit v1.1

