From 5d92ae4eb6fa1ad70e953e6fdbbf6dcc5831b5b4 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C3=ABl=20Carr=C3=A9?= <rafael.carre@gmail.com>
Date: Thu, 20 May 2010 19:58:45 +0000
Subject: manual: change all references to 'headphone jack' into more correct
 'headphone socket'

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@26213 a1c6a512-1295-4272-9138-f99709370657
---
 manual/rockbox_interface/main.tex | 20 ++++++++++----------
 1 file changed, 10 insertions(+), 10 deletions(-)

(limited to 'manual/rockbox_interface/main.tex')

diff --git a/manual/rockbox_interface/main.tex b/manual/rockbox_interface/main.tex
index 95c21f4..50d41c8 100644
--- a/manual/rockbox_interface/main.tex
+++ b/manual/rockbox_interface/main.tex
@@ -99,10 +99,10 @@ detail in the following paragraph.
 
   The top of the player will have the following, from left to 
   right:
-  \opt{ipod4g,ipodcolor}{remote connector, headphone jack, \ButtonHold{} 
+  \opt{ipod4g,ipodcolor}{remote connector, headphone socket, \ButtonHold{} 
     switch.}
-  \opt{ipodvideo}{\ButtonHold{} switch, headphone jack.}
-  \opt{ipodmini}{\ButtonHold{} switch, remote connector, headphone jack.}	
+  \opt{ipodvideo}{\ButtonHold{} switch, headphone socket.}
+  \opt{ipodmini}{\ButtonHold{} switch, remote connector, headphone socket.}	
 
   The dock connector that is used to connect your \dap{} to your computer is on 
   the bottom panel of the \dap{}.
@@ -128,7 +128,7 @@ detail in the following paragraph.
   facing you. 
 
   The top of the player will have the following, from left to 
-  right: remote connector, headphone jack, \ButtonHold{} switch.
+  right: remote connector, headphone socket, \ButtonHold{} switch.
 	
   The dock connector that is used to connect your \dap{} to your computer is on 
   the bottom panel of the \dap{}.
@@ -155,7 +155,7 @@ detail in the following paragraph.
   facing you. 
 
   The top of the player will have the following, from left to 
-  right: FireWire port, headphone jack, \ButtonHold{} switch.
+  right: FireWire port, headphone socket, \ButtonHold{} switch.
 
   The FireWire port is used to connect your \dap{} to the computer and
   to charge its battery via a wall charger.
@@ -200,7 +200,7 @@ detail in the following paragraph.
   which is the MMC slot. Holding the \dap{} with this slot in the described position
   you'll find the following:
 
-  On the curved top, from left to right, are the headphone jack,
+  On the curved top, from left to right, are the headphone socket,
   the \ButtonOff{} button,%
   \opt{recording}{ and the line-in jack}.
   Apart from the already mentioned MMC slot, you will find the USB connector on
@@ -381,7 +381,7 @@ detail in the following paragraph.
   On the lower left of the unit is a slot for inserting microSD cards. Immediately below that is
   the opening for the microphone.
 
-  On the bottom of the unit is the connector for connecting a USB cable and the headphone jack.
+  On the bottom of the unit is the connector for connecting a USB cable and the headphone socket.
   On the lower right hand side of the unit is a two-way switch. Pressing this switch up acts as
   \ButtonPower{}, and clicking it down until it locks acts as the \ButtonHold{} switch. When the
   \ButtonHold{} switch is on, none of the other buttons have any effect.
@@ -416,7 +416,7 @@ detail in the following paragraph.
 
   On the right hand panel is a two-way button that acts as \ButtonVolDown{} when
   pressed on the bottom, and \ButtonVolUp{} when pressed on the top. Immediately
-  above this button is the headphone jack.
+  above this button is the headphone socket.
   }
   %
   \opt{vibe500}{
@@ -449,7 +449,7 @@ detail in the following paragraph.
   button on the right contains, clockwise from the top, the \ButtonPlay{},
   the \ButtonRight{}, the \ButtonStop{}, and the \ButtonLeft{} buttons.
 
-  On the top on the \dap{} is the headphone jack on the left and the line-out
+  On the top on the \dap{} is the headphone socket on the left and the line-out
   jack on the right. On the bottom of the \dap{} is the line-in jack on the left,
   the DC-In jack on the right, and the USB connector in the centre.
   }
@@ -471,7 +471,7 @@ detail in the following paragraph.
   of three rectangular buttons the following buttons can be found (from left to right):
   \ButtonFOne{}, \ButtonFTwo{} and \ButtonFThree{}.
 
-  On the top of the \dap{} is the headphone jack on the left and the line-out jack on
+  On the top of the \dap{} is the headphone socket on the left and the line-out jack on
   the right. On the bottom of the \dap{} is the line-in jack on the left, the
   DC-In jack on the right, and the USB connector in the centre.
   }
-- 
cgit v1.1

