From 53cf63fbbc3a8b0d41feb7b81c1ef0da652f616b Mon Sep 17 00:00:00 2001
From: Andree Buschmann <AndreeBuschmann@t-online.de>
Date: Wed, 14 Apr 2010 19:44:07 +0000
Subject: Consistent use of Hz, kHz, dB, dbFS, ms, s and min. Add spaces
 between number and unit -- e.g. '5 dB'.

git-svn-id: svn://svn.rockbox.org/rockbox/trunk@25648 a1c6a512-1295-4272-9138-f99709370657
---
 manual/appendix/appendix.tex | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

(limited to 'manual/appendix/appendix.tex')

diff --git a/manual/appendix/appendix.tex b/manual/appendix/appendix.tex
index 2130a0e..99bc626 100644
--- a/manual/appendix/appendix.tex
+++ b/manual/appendix/appendix.tex
@@ -73,7 +73,7 @@ The recording hardware (the MAS) does not allow us to do this
   The mp3{}-decoding hardware cannot decode OGG. It can be reprogrammed, but 
   there is too little memory for OGG and we have no documentation on how to 
   program the MAS' DSP. Doing the conversion with the CPU is impossible, since 
-  a 12MHz SH1 is far too slow for this daunting task.
+  a 12 MHz SH1 is far too slow for this daunting task.
 \item Archos Multimedia support.\\
   The Archos Multimedia is a completely different beast. It is an entirely 
   different architecture, different CPU and upgrading the software is done 
-- 
cgit v1.1

